Module M Test Hand Tools, tcfh2-3-14, rev1.0,

This is the test. Complete the test for 0.5 hours credit in the Safety and Loss Prevention program. Email the test to billy.ernst@angeltrax .com. A 100% score earns 0.5 hours credit.

TOOLS: HAND

[**General requirements. - 1926.300**](http://www.osha.gov/pls/oshaweb/owadisp.show_document?p_table=STANDARDS&amp;p_id=10688)[**Hand tools. - 1926.301**](http://www.osha.gov/pls/oshaweb/owadisp.show_document?p_table=STANDARDS&amp;p_id=10689)

When using hand and power tools, appropriate       will be used to provide protection for the eyes, skin, ears, hands, feet, and respiratory system in accordance with our PPE Program located in Section III.

Any tool not in compliance with OSHA or ANSI standards will not be used. Such tools, as well as any tools found to be defective in any manner, will be identified as      by       and removed from the job site.

All tools, whether company or employee owned, will be maintained in a       condition.

Hand tools shall be used only for the       for which they are designed. Hand tools will be kept       and, where appropriate, oiled.

Hand tools which are       will not be used.

Hand held       tools will be kept sharp and will be sheathed or retracted when not in use.

When using a striking tool such as a hammer or chisel, safety       or safety       will be used.

Do not force tools.

If you are unfamiliar with the proper procedure for using a tool, ask your       for instruction.

Power tools may be operated only by those persons who are       by training or experience.

Guards will be used on power tools. Under no circumstances will       be by-passed or altered.

Electrical tools must be grounded and, in the absence of permanent wiring, a      must be used.

Electric tools will not be       by their cords and pneumatic tools will not be      by their hoses.